|  |  |
| --- | --- |
| **Исходный текст** | **Перевод** |
| Running maintenance  During operation, if suffered agglomerate over disintegrator load or big block sundries to build up, reverse disgorge three times continually and still cannot pass, clean them after reversion by manpower hand and let entering garbage uniform. During operation, generator operate normally and blade bearing is still, the reason is that overloading leads to safety bolt cut out. Replace overloading safety bolt. Roller bearing is full life lubrication under no leakage after filling lubricating grease at a time, and does not need to oil. | Повседневное обслуживание  В процессе работы, при попадании крупных фрагментов или образовании пробки, переведите измельчитель на обратный режим вращения для освобождения загрузочной емкости. Если после трех попыток удалить пробку не получилось, удалите ее вручную и следите за тем, чтобы загружаемый мусор не содержал крупных фрагментов.  Во время работы двигатель работает нормально, но измельчающее колесо не вращается. Возможно произошло срезание предохранительного болта вследствие перегрузки. Замените предохранительный болт. Шарикоподшипник является маслонаполненным и не требует дополнительной смазки в процессе эксплуатации. |