|  |  |
| --- | --- |
| Оригинал | Перевод |
| **Before use**  The appliance may only be used for the intended purpose according to these operating instructions.  For this reason, please read the instruction manual carefully before use as it provides instructions for using, cleaning and caring for the appliance. We accept no liability for any damages caused if this manual is not observed. Keep the operating manual in a safe place and pass it on to any subsequent user together with the appliance.  Observe the safety information when using the appliance.  **Technical data**  Rated voltage: 220–240 V~ 50–60 Hz  Power consumption: 900 W  Protection class: I  **Additional safety information**  ▪▪ Only connect the appliance to earthed wall sockets that have been installed pursuant to regulations. The supply cable and plug must be dry.  ▪▪ Do not pull or clamp the connecting cable over sharp edges. Do not leave it dangling and protect it from heat and oil.  ▪▪ Only use an extension cable that is in perfect condition.  ▪▪ Never pull the mains plug out of the socket by the cable or with wet hands. | **Перед использованием**  Прибор можно использовать исключительно в соответствии с его назначением согласно данному руководству по эксплуатации. В этой связи, пожалуйста, внимательно ознакомьтесь с руководством по эксплуатации перед использованием, так как оно содержит инструкции по использованию, чистке и уходу за прибором. Мы не несем ответственности за какой-либо ущерб, вызванный несоблюдением данного руководства. Храните руководство по эксплуатации в надежном месте и передавайте его всем последующим пользователям вместе с прибором. Соблюдайте правила техники безопасности при использовании прибора.  **Технические характеристики**  Номинальное напряжение: 220–240 В ~ 50–60 Гц  Потребляемая мощность: 900 Вт  Степень защиты: I  **Дополнительная информация по безопасности**  **▪ ▪** Подключайте прибор только к заземленным розеткам, установленным в соответствии с правилами. Кабель питания и вилка должны быть сухими.  ▪ ▪ Не протягивайте и не зажимайте соединительный кабель между острыми краями. Не оставляйте кабель незафиксированным и защищайте от воздействия тепла и масла.  ▪ ▪ Используйте только тот удлинительный кабель, который находится в идеальном состоянии.  **▪ ▪** Никогда не вынимайте вилку из розетки, держась за кабель, или мокрыми руками. |